**Custom PedalSnake Order Menu**

**Directions (see** [**About Custom PedalSnakes**](http://www.pedalsnake.com/dev/page.php?id=18)**)**

* To purchase, you must first approve our quote. To receive a quote, fill out and [email](mailto:sales2@pedalsnake.com?subject=My%20Rig%20Questionnaire) this form back to [sales2@pedalsnake.com](mailto:sales2@pedalsnake.com)
* **Do not alter table formatting.** Just enter your info into each box.

|  |  |  |  |
| --- | --- | --- | --- |
| **First** |  | **State** |  |
| **Last** |  | **Zipcode** |  |
| **Company** |  | **Country** |  |
| **Address 1** |  | **Email** |  |
| **Address 2** |  | **Phone** |  |
| **City** |  |  |  |

**Filling Out the Options Table**

* Save this form on your computer. Name it with your last name, like “Axman CustomCS.doc”.
* Save and return it as an attachment to this [email](mailto:sales2@pedalsnake.com?subject=Custom%20PedalSnake%20Quote) to [sales2@pedalsnake.com](mailto:sales2@pedalsnake.com).
  + We recommend you choose at least some[**plug’n’play DIN channels**](http://www.pedalsnake.com/page.php?id=64#chOverview)(3wire and 5wire)that can be configured with[**pigtails**](http://www.pedalsnake.com/page.php?id=64#Pigtails), in case your rig changes.
  + **NOTE** We have 4 and 8-paircable. Some channels require more than 1 pair (see below). Any pairs you don’t require are chopped off and go unseen.
* Payment via credit card and PayPal (preferred). **For obvious reasons, all custom sales are final.**
* Enter numbers in the **green “qty” column** to show what you need:

|  |  |
| --- | --- |
| **Total Length** | Total length of the cable in FEET, including the stripped-back part for fanouts at both ends. |
| **Fans** | Length of the stripped back part in INCHES, exposing the “pairs”. See [Fanout Length](http://www.pedalsnake.com/page.php?id=1115#fanLength). |
| **DIN Channels** | Specify how many of each type DIN channel (3wire and 5wire are configurable with Pigtails) |
| **¼” Lines** | BLUE letter = Pedal End, RED letter = Amp End; R=right-angle plug, S=straight plug |
| **XLR Lines** | BLUE letter = Pedal End, RED letter = Amp End; F=female M=male |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Lengths** | **qty** | **units** | **range** | **description** |
| Total Length | 0 | feet | 4-30’ | Total length, includes fans (try 4 ft for racks!) |
| PedalEnd Fan | 0 | inches | 6-48” | To reach all pedals (18” typical) |
| AmpEnd Fan | 0 | inches | 6-48” | To reach between amps, racks, etc. (24” typical) |
| **DIN Channels** |  | **pairs used** | **description** | |
| 3-wire | 0 | 1 | 5pin DIN connector, 3 pins wired, accepts Pigtails | |
| 5-wire | 0 | 2 | 5pin DIN connector, 5 pins wired, accepts Pigtails | |
| 7-wire | 0 | 3 | 7pin DIN connector, 7 pins wired | |
| **Hardwired ¼” G-Lines** |  | **pairs used** | **description** | |
| RS | 0 | 1 | 1/4” mono line, right-angle at Pedal End only | |
| SS | 0 | 1 | 1/4” mono line, straight at both ends | |
| SR | 0 | 1 | 1/4” mono line, right-angle at Amp End only | |
| RR | 0 | 1 | 1/4” mono line, right-angle at both ends | |
| TRS | 0 | 1 | 1/4” stereo line, straight TRS (tip-ring-sleeve) at both ends | |
| **XLR Lines** |  |  |  | |
| XFM ­­­ | 0 | 1 | Female at Pedal End, Male at Amp End | |
| XMF | 0 | 1 | Male at Pedal End, Female at Amp End | |

**Custom PedalSnake Costs Explained**

**Retail Prices Shown**

Cable Costs

# Custom PedalSnake models are made from multi-pair cable. We have 2 different multi-pair cables:

**Cable Size Cost/Foot Cable Type**

4-pair 1.38 IJ (Individually Jacketed), each pair with a unique color

8-pair 2.67 IJ (Individually Jacketed); each pair with a unique color

**NOTE** All lines and channels that you order will use 1 pair in the cable, except for:

* + 5wire channel (uses 2 pairs)
  + 7wire channel (uses 3 pairs).

Channel and Line Costs (parts and labor)

This is the cost of the plugs and labor required to convert a bare cable wire-pair into a functional channel or line. Note that the cost varies according to whether the cable type is IJ or NIJ.

3-wire 14.85

5-wire 25.65

7-wire 36.45

Any ¼” Line 13.50

Any XLR Line 13.50

# Fanout Costs

12–24" Free

30–48” Fanout Upcharge (for fans over 24”): $0.54 per end, per line, per 6" over 24".

*Example*  *5-line PedalSnake, fans: 24” Pedal End, 36” Amp End*

*Pedal End No upcharge*

*Amp End $5.40 Upcharge = 1 (end) x 5 (lines) x 2 (6” increments beyond 24”) x $0.54*

Design Fee

20.00

This covers the:

* Review of your Custom Menu choices, and submittal of your Custom PedalSnake to our manufacturer.
* The shipping costs from the manufacturer to Stage Magic Inc. (us).
* Our inspection of your Custom PedalSnake before shipping to you.